{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[1,1,1,5]]}
[null,"附件"]
[null,"泉州市光前医院2026年定点采购监控设备招标报价单"]
[null,"序号","名称","主要参数","单位","单价"]
[null,1,"室内一体化球机","400万像素，带拾音器接口。采用1/1.8”C1OS，LED红外50-100米，内置GFU芯片，支持深度学习算法，支持四种智能资源切换:通用行为分析、人脸检测、视频结构化、人数统计。支持DC12V/AC24V/POE供电方式，IP67防护等级","台"]
[null,2,"网络半球摄像机","400万像素带拾音器接口。1/2.8”CMOS，LED红外10-30米，microSD， DC12V/PoE(802.3af)，IF66，IK10防暴，背光补偿，数字宽动态，ROI，配套腾装支架2.8/4/6/8/12mm镜头可选，支持128G","台"]
[null,3,"网络枪式摄像机","400万像素，带拾音器接口，1/2.8”cmos，配护器和镜头，LED红外10-50米，4/6/8/12m镜头可选支持128G micro SD.DC12V/PoE(802.3af)，IP66，背光补偿，数字宽动态， ROI","台"]
[null,4,"电梯专用摄像机","400万像责，带拾音恭接口，1/3”CMOS，LED红外10米，2.8/4/6镜头可选，背光补偿，数字宽动态。ROI，支持128Gmicro SDDC12V/PoE(802.3af)","台"]
[null,5,"室外球机","400万/智能运动眼眯/越界侦测、区域入侵、移动侦测、视规遮挡侦测，ROI/IF66/红外200米,配护、云台、5m立杆镀锌钢管喷漆支架、配避雪针交接箱","台"]
[null,6,"拾音器","内置音频采生模块，智能破音保护，具备啸叫抑制功能。内置CPU，实时处理声音信号，延时小，大量雪击保护，由返极性反接保护和静由保护，符和ROHS标准。","只"]
[null,7,"光纤收发器","1个10/100/1000BaseT(X)自适应RJ45 LAN口:1个1000BaseX以太网光纤楼口，单模单纤","对"]
[null,8,"硬盘录像机","可接驳符合ONVIF、RTSP标准的众多主流厂商网络摄像机；支持接入H.265、Smart265、H.264、Smart264视频编码码流；支持800万像素高清网络视频的预览、存储与回放；自带4个SATA接口，最大支持满配10T硬盘","台"]
[null,9,"硬盘","企业级8TB","块"]
[null,10,"POE接入交换机","万兆上行交换机, 传输速率转发能力 65.7Mpps , 端口结构固定端口 24个10/100/1000Base-T电口(包含两个uplink口，可作为上行口)，2个10G Base-X SFP+ 光口","台"]
[null,11,"POE接入交换机","8个千兆电口+2个千兆上联电口，其中8个口支持PoE/PoE+供电，最大PoE功率57W，交换容量：20Gbps，包转发率：14.9Mpps","台"]
[null,12,"非屏蔽双绞线","六类4对非屏蔽，无氧铜,160M带电传输零差损","米"]
[null,13,"8芯单模光缆","电信级,支持万兆传输能力，曲径小于10mm,差损小于0.02dB","米"]
[null,14,"室外防水机柜","天恒400*500","个"]
[null,15,"线管","冠益管道","米"]
[null,16,"无线网桥","腾达01-5G","套"]
[null,17,"排插","公牛6插位","个"]
[null,18,"摄像机支架",null,"个"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}